Mejuffrou Rak – Installation guide

What you will need:

⮚ 6mm masonry drill bit

⮚10mm masonry drill bit

⮚14mm masonry drill bit

⮚Drill

⮚Level

⮚Rubber hammer

⮚Pencil

⮚Tape measure

**STEP 1:**

Make sure that there are no water pipes or electric cables in the wall where you want to install the shelves.

**STAP 2:**

Hold the level against the wall where you want the shelf to be and draw a line with the pencil. Use the tape measure and draw marks where the holes should be.

**STAP 3:**

Drill the holes starting with the 6mm drill bit. Next, use the 10mm drill bit to drill the holes bigger. Lastly, use the 14mm for the final size. The hole should be 75mm deep. By using the various drill bits, it prevents the plaster on walls to break roughly.

**STEP 4:**

Place the brackets in the holes. Use the rubber hammer to get the brackets deeper into the holes. Turn the brackets clockwise until tight.

**STEP 5:**

Push the shelf onto the brackets making sure the brackets go into the holes.

**STEP 6:**

Enjoy the convenience of your shelf and don’t forget to let us know of any problems that you might experience. Please feel free to write a review on our Facebook-page.